
8,16,2017

Try to disable the enter SLEEP mode of the MCU, disable ‘EMU\_EnterEM2’

Try to disable the enter SLEEP mode of the DWM1000, disable ‘DWM1000\_enter\_sleepmode()’,’DWM1000\_SPI\_Wake\_Up (wakeup\_buffer, 50)’, ‘DWM1000\_enter\_sleepmode()’

Try to disable cc1101\_power\_down, ‘cc1101\_power\_down()’

Don’t work

0a070bf8edb68461c50ed8a8d61ac901bf76a690 modified AS3933.c in node making it more reliable, namely less chance to return 0 data; 

Trying to do the same to the tag

Besides the command send from the base looks like thereis problem, since sometime false returned here in AS3933.c

