Trimmean()

Mad()

Plot of errors(mean variance) to #nodes actived in the last n seconds

Root mean square of derivation from the true trajectory of EKF

Calibration-Free Localization.m >>

set rand factor for gamma seems could solve local minimal problem :D