8,16,2017

Try to disable the enter SLEEP mode of the MCU, disable ‘EMU\_EnterEM2’

Try to disable the enter SLEEP mode of the DWM1000, disable ‘DWM1000\_enter\_sleepmode()’,’DWM1000\_SPI\_Wake\_Up (wakeup\_buffer, 50)’, ‘DWM1000\_enter\_sleepmode()’

Try to disable cc1101\_power\_down, ‘cc1101\_power\_down()’